Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetLaserWakeupEncoderTravel | ( | GoSetup | setup,
|  | k64u | distance
| ) |  |

This API is experimental and may change in a future release Sets the encoder wakeup travel distance.

Version
  Introduced in firmware 4.8.2.76

Parameters

  setup | GoSetup object.
  distance | distance (mm)

Returns
  Operation status.