Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k64f GoSetup_BackCameraExposureLimitMax | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the maximum valid value for the back camera exposure setting.

Version
  Introduced in firmware 4.6.0.140

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from.

Returns
  Maximum valid auxiliary exposure value (microseconds).