Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoSensor Member List

This is the complete list of members for GoSensor, including all inherited members.

GoSensor_AddBuddy(GoSensor sensor, GoSensor buddy) | GoSensor |
GoSensor_AddBuddyBlocking(GoSensor sensor, GoSensor buddy) | GoSensor |
GoSensor_Address(GoSensor sensor, GoAddressInfo *info) | GoSensor |
GoSensor_Align(GoSensor sensor) | GoSensor |
GoSensor_AlignmentReference(GoSensor sensor, GoAlignmentRef *reference) | GoSensor |
GoSensor_AlignmentState(GoSensor sensor) | GoSensor |
GoSensor_AutoStartEnabled(GoSensor sensor) | GoSensor |
GoSensor_Backup(GoSensor sensor, const kChar *destPath) | GoSensor |
GoSensor_BuddiesCount(GoSensor info) | GoSensor |
GoSensor_BuddyId(GoSensor sensor) | GoSensor |
GoSensor_Cancel(GoSensor sensor) | GoSensor |
GoSensor_ChangePassword(GoSensor sensor, GoUser user, const kChar *password) | GoSensor |
GoSensor_ClearAlignment(GoSensor sensor) | GoSensor |
GoSensor_ClearLog(GoSensor sensor) | GoSensor |
GoSensor_ClearMeasurementStats(GoSensor sensor) | GoSensor |
GoSensor_ClearReplayData(GoSensor sensor) | GoSensor |
GoSensor_Connect(GoSensor sensor) | GoSensor |
GoSensor_ControlPort(GoSensor sensor) | GoSensor |
GoSensor_CopyFile(GoSensor sensor, const kChar *sourceName, const kChar *destName) | GoSensor |
GoSensor_DataPort(GoSensor sensor) | GoSensor |
GoSensor_DefaultJob(GoSensor sensor, kChar *fileName, kSize capacity) | GoSensor |
GoSensor_DeleteFile(GoSensor sensor, const kChar *name) | GoSensor |
GoSensor_DirectoryFileCount(GoSensor sensor, const kChar *extensionFilter, const kChar *path, kBool isRecursive) | GoSensor |
GoSensor_DirectoryFileNameAt(GoSensor sensor, const kChar *extensionFilter, const kChar *path, kBool isRecursive, kSize index, kChar *fileName, kSize capacity) | GoSensor |
GoSensor_Disconnect(GoSensor sensor) | GoSensor |
GoSensor_DownloadFile(GoSensor sensor, const kChar *sourceName, const kChar *destPath) | GoSensor |
GoSensor_EmitAnalog(GoSensor sensor, k16u index, k64s target, k32s value) | GoSensor |
GoSensor_EmitDigital(GoSensor sensor, k16u index, k64s target, k8u value) | GoSensor |
GoSensor_EnableAutoStart(GoSensor sensor, kBool enable) | GoSensor |
GoSensor_EnableData(GoSensor sensor, kBool enable) | GoSensor |
GoSensor_EnableQuickEdit(GoSensor sensor, kBool enable) | GoSensor |
GoSensor_EnableRecording(GoSensor sensor, kBool enable) | GoSensor |
GoSensor_Encoder(GoSensor sensor, k64s *encoder) | GoSensor |
GoSensor_ExportBitmap(GoSensor sensor, GoReplayExportSourceType type, GoDataSource source, const kChar *dstFileName) | GoSensor |
GoSensor_ExportCsv(GoSensor sensor, const kChar *dstFileName) | GoSensor |
GoSensor_ExposureAutoSet(GoSensor sensor, GoRole role) | GoSensor |
GoSensor_Family(GoSensor sensor) | GoSensor |
GoSensor_FileCount(GoSensor sensor) | GoSensor |
GoSensor_FileExists(GoSensor sensor, const kChar *name) | GoSensor |
GoSensor_FileNameAt(GoSensor sensor, kSize index, kChar *name, kSize capacity) | GoSensor |
GoSensor_FirmwareVersion(GoSensor sensor) | GoSensor |
GoSensor_GeoCal(GoSensor info, GoGeoCal *geoCal) | GoSensor |
GoSensor_GetRuntimeVariableAt(GoSensor sensor, kSize index, k32s *value) | GoSensor |
GoSensor_GetRuntimeVariableCount(GoSensor sensor) | GoSensor |
GoSensor_GetRuntimeVariables(GoSensor sensor, kSize startIndex, kSize length, k32s *values) | GoSensor |
GoSensor_GetVoltage(GoSensor sensor, GoVoltageSetting *voltage, k64f *cableLength) | GoSensor |
GoSensor_HasBuddies(GoSensor info) | GoSensor |
GoSensor_HasBuddy(GoSensor sensor) | GoSensor |
GoSensor_HealthPort(GoSensor sensor) | GoSensor |
GoSensor_Id(GoSensor sensor) | GoSensor |
GoSensor_InputSource(GoSensor sensor) | GoSensor |
GoSensor_IsCompatible(GoSensor sensor) | GoSensor |
GoSensor_IsConnected(GoSensor sensor) | GoSensor |
GoSensor_IsRecordingStreaming(GoSensor sensor) | GoSensor |
GoSensor_IsResponsive(GoSensor sensor) | GoSensor |
GoSensor_LoadedJob(GoSensor sensor, kChar *fileName, kSize capacity, kBool *changed) | GoSensor |
GoSensor_LogIn(GoSensor sensor, GoUser user, const kChar *password) | GoSensor |
GoSensor_Model(GoSensor sensor, kChar *model, kSize capacity) | GoSensor |
GoSensor_Output(GoSensor sensor) | GoSensor |
GoSensor_PartMatchCreateModel(GoSensor sensor, const kChar *name) | GoSensor |
GoSensor_PartMatchDetectModelEdges(GoSensor sensor, const kChar *name, k16u sensitivity) | GoSensor |
GoSensor_PartMatchModel(GoSensor sensor, const kChar *name) | GoSensor |
GoSensor_PartMatchModelAt(GoSensor sensor, kSize index) | GoSensor |
GoSensor_PartMatchModelCount(GoSensor sensor) | GoSensor |
GoSensor_PlaybackPosition(GoSensor sensor, kSize *position, kSize *count) | GoSensor |
GoSensor_PlaybackSeek(GoSensor sensor, kSize position) | GoSensor |
GoSensor_PlaybackStep(GoSensor sensor, GoSeekDirection direction) | GoSensor |
GoSensor_ProtocolVersion(GoSensor sensor) | GoSensor |
GoSensor_QuickEditEnabled(GoSensor sensor) | GoSensor |
GoSensor_RecordingEnabled(GoSensor sensor) | GoSensor |
GoSensor_Refresh(GoSensor sensor) | GoSensor |
GoSensor_RemoteInfoAt(GoSensor sensor, kSize index) | GoSensor |
GoSensor_RemoteInfoCount(GoSensor sensor) | GoSensor |
GoSensor_RemoveBuddy(GoSensor sensor) | GoSensor |
GoSensor_Replay(GoSensor sensor) | GoSensor |
GoSensor_Reset(GoSensor sensor, kBool wait) | GoSensor |
GoSensor_ResetEncoder(GoSensor sensor) | GoSensor |
GoSensor_Restore(GoSensor sensor, const kChar *sourcePath) | GoSensor |
GoSensor_RestoreDefaults(GoSensor sensor, kBool restoreAddress) | GoSensor |
GoSensor_Role(GoSensor sensor) | GoSensor |
GoSensor_ScanMode(GoSensor sensor) | GoSensor |
GoSensor_ScheduledStart(GoSensor sensor, k64s value) | GoSensor |
GoSensor_SetAddress(GoSensor sensor, const GoAddressInfo *info, kBool wait) | GoSensor |
GoSensor_SetAlignmentReference(GoSensor sensor, GoAlignmentRef reference) | GoSensor |
GoSensor_SetControlPort(GoSensor sensor, k32u port) | GoSensor |
GoSensor_SetDataHandler(GoSensor sensor, GoSensorDataSetFx function, kPointer context) | GoSensor |
GoSensor_SetDataPort(GoSensor sensor, k32u port) | GoSensor |
GoSensor_SetDefaultJob(GoSensor sensor, const kChar *fileName) | GoSensor |
GoSensor_SetHealthPort(GoSensor sensor, k32u port) | GoSensor |
GoSensor_SetInputSource(GoSensor sensor, GoInputSource source) | GoSensor |
GoSensor_SetRuntimeVariables(GoSensor sensor, kSize startIndex, kSize length, k32s *values) | GoSensor |
GoSensor_Setup(GoSensor sensor) | GoSensor |
GoSensor_SetUpgradePort(GoSensor sensor, k32u port) | GoSensor |
GoSensor_SetVoltage(GoSensor sensor, GoVoltageSetting voltage, k64f cableLength) | GoSensor |
GoSensor_Simulate(GoSensor sensor, kBool *isBufferValid) | GoSensor |
GoSensor_Start(GoSensor sensor) | GoSensor |
GoSensor_StartRecordingStream(GoSensor sensor, kChar *destFile) | GoSensor |
GoSensor_State(GoSensor sensor) | GoSensor |
GoSensor_States(GoSensor sensor, GoStates *states) | GoSensor |
GoSensor_Stop(GoSensor sensor) | GoSensor |
GoSensor_StopRecordingStream(GoSensor sensor) | GoSensor |
GoSensor_Timestamp(GoSensor sensor, k64u *time) | GoSensor |
GoSensor_Tools(GoSensor sensor) | GoSensor |
GoSensor_Transform(GoSensor sensor) | GoSensor |
GoSensor_Trigger(GoSensor sensor) | GoSensor |
GoSensor_Upgrade(GoSensor sensor, const kChar *sourcePath, GoUpgradeFx onUpdate, kPointer context) | GoSensor |
GoSensor_UpgradePort(GoSensor sensor) | GoSensor |
GoSensor_UploadFile(GoSensor sensor, const kChar *sourcePath, const kChar *destName) | GoSensor |
GoSensor_User(GoSensor sensor) | GoSensor |
GoSensor_UserStorageFree(GoSensor sensor) | GoSensor |
GoSensor_UserStorageUsed(GoSensor sensor) | GoSensor |
GoSensorDataSetFx typedef | GoSensor |
GoSystem_GetExtendedDiscoveryInfo(GoSystem system, k32u deviceId, GoDiscoveryExtInfo *info, kAlloc allocator) | GoSensor |