Gocator API

- Home
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
GoSerial.h
Go to the documentation of this file.
1 /**
2 * @file GoSerial.h
3 * @brief Declares the GoSerial class.
4 *
5 * @internal
6 * Copyright (C) 2016-2018 by LMI Technologies Inc.
7 * Licensed under the MIT License.
8 * Redistributed files must retain the above copyright notice.
9 */
10 #ifndef GO_SDK_SERIAL_H
11 #define GO_SDK_SERIAL_H
12
13 #include <GoSdk/GoSdkDef.h>
14 kBeginHeader()
15
16 /**
17 * @class GoSerial
18 * @extends kObject
19 * @ingroup GoSdk-Serial
20 * @brief Represents Serial output settings.
21 */
22 typedef kObject GoSerial;
23
24 /**
25 * Gets the count of serial protocol options.
26 *
27 * @public @memberof GoSerial
28 * @version Introduced in firmware 4.1.3.106
29 * @param serial GoSerial object.
30 * @return Protocol option.
31 */
32 GoFx(kSize) GoSerial_ProtocolOptionCount(GoSerial serial);
33
34 /**
35 * Gets the serial protocol option at the specified index.
36 *
37 * @public @memberof GoSerial
38 * @version Introduced in firmware 4.1.3.106
39 * @param serial GoSerial object.
40 * @param index Protocol option index.
41 * @return Protocol option.
42 */
43 GoFx(k32u) GoSerial_ProtocolOptionAt(GoSerial serial, kSize index);
44
45 /**
46 * Sets the Serial output protocol.
47 *
48 * @public @memberof GoSerial
49 * @version Introduced in firmware 4.1.3.106
50 * @param serial GoSerial object.
51 * @param protocol Protocol option value;
52 * @return Operation status.
53 * @see GoSerial_ProtocolOptionCount, GoSerial_ProtocolOptionAt
54 */
55 GoFx(kStatus) GoSerial_SetProtocol(GoSerial serial, k32u protocol);
56
57 /**
58 * Returns the current Serial output protocol value.
59 *
60 * @public @memberof GoSerial
61 * @version Introduced in firmware 4.1.3.106
62 * @param serial GoSerial object.
63 * @return An integer corresponding to the current Serial output protocol.
64 */
65 GoFx(k32u) GoSerial_Protocol(GoSerial serial);
66
67 /**
68 * Gets the number of source options.
69 *
70 * @public @memberof GoSerial
71 * @version Introduced in firmware 4.0.10.27
72 * @param serial GoSerial object.
73 * @return Source option.
74 */
75 GoFx(kSize) GoSerial_OptionCount(GoSerial serial);
76
77 /**
78 * Gets the source option at the specified index.
79 *
80 * @public @memberof GoSerial
81 * @version Introduced in firmware 4.0.10.27
82 * @param serial GoSerial object.
83 * @param index Source option index.
84 * @return Source option.
85 */
86 GoFx(k32u) GoSerial_OptionAt(GoSerial serial, kSize index);
87
88 /**
89 * Gets the number of sources of the specified output type that are currently selected for transmission.
90 *
91 * @public @memberof GoSerial
92 * @version Introduced in firmware 4.0.10.27
93 * @param serial GoSerial object.
94 * @return Count of selected sources.
95 */
96 GoFx(kSize) GoSerial_SourceCount(GoSerial serial);
97
98 /**
99 * Gets the identifier of the selected output source at the specified index.
100 *
101 * @public @memberof GoSerial
102 * @version Introduced in firmware 4.0.10.27
103 * @param serial GoSerial object.
104 * @param index Selected source index.
105 * @return Source identifier.
106 */
107 GoFx(k32u) GoSerial_SourceAt(GoSerial serial, kSize index);
108
109 /**
110 * Selects the specified source for transmission.
111 *
112 * @public @memberof GoSerial
113 * @version Introduced in firmware 4.0.10.27
114 * @param serial GoSerial object.
115 * @param sourceId Source identifier.
116 * @return Operation status.
117 */
118 GoFx(kStatus) GoSerial_AddSource(GoSerial serial, k32u sourceId);
119
120 /**
121 * Removes (de-selects) the source at the specified index.
122 *
123 * @public @memberof GoSerial
124 * @version Introduced in firmware 4.0.10.27
125 * @param serial GoSerial object.
126 * @param index Index of the source to be removed.
127 * @return Operation status.
128 */
129 GoFx(kStatus) GoSerial_RemoveSource(GoSerial serial, kSize index);
130
131 /**
132 * Removes all selected sources for the specified output type.
133 *
134 * @public @memberof GoSerial
135 * @version Introduced in firmware 4.0.10.27
136 * @param serial GoSerial object.
137 * @return Operation status.
138 */
139 GoFx(kStatus) GoSerial_ClearSources(GoSerial serial);
140
141 /**
142 * Sets the Selcom protocol output rate.
143 *
144 * @public @memberof GoSerial
145 * @version Introduced in firmware 4.0.10.27
146 * @param serial GoSerial object.
147 * @param rate The Selcom rate to use.
148 * @return Operation status.
149 * @see GoSerial_SelcomRateOptionCount, GoSerial_SelcomRateOptionAt
150 */
151 GoFx(kStatus) GoSerial_SetSelcomRate(GoSerial serial, k32u rate);
152
153 /**
154 * Gets the index of the currently selected Selcom output rate.
155 *
156 * @public @memberof GoSerial
157 * @version Introduced in firmware 4.0.10.27
158 * @param serial GoSerial object.
159 * @return An integer corresponding to the current Selcom output rate.
160 */
161 GoFx(k32u) GoSerial_SelcomRate(GoSerial serial);
162
163 /**
164 * Gets the list of Selcom rate options.
165 *
166 * @public @memberof GoSerial
167 * @version Introduced in firmware 4.0.10.27
168 * @param serial GoSerial object.
169 * @return An array list of Selcom rate options.
170 */
171 GoFx(kArrayList) GoSerial_SelcomRateOptionList(GoSerial serial);
172
173 /**
174 * Returns the count of available Selcom protocol output rate options.
175 *
176 * @public @memberof GoSerial
177 * @version Introduced in firmware 4.0.10.27
178 * @param serial GoSerial object.
179 * @return Count of available Selcom protocol output rate options.
180 */
181 GoFx(kSize) GoSerial_SelcomRateOptionCount(GoSerial serial);
182
183 /**
184 * Gets the Selcom rate option at the specified index.
185 *
186 * @public @memberof GoSerial
187 * @version Introduced in firmware 4.0.10.27
188 * @param serial GoSerial object.
189 * @param index Selcom rate option index.
190 * @return Selcom rate option value.
191 */
192 GoFx(k32u) GoSerial_SelcomRateOptionAt(GoSerial serial, kSize index);
193
194 /**
195 * Sets the Selcom protocol output format.
196 *
197 * @public @memberof GoSerial
198 * @version Introduced in firmware 4.0.10.27
199 * @param serial GoSerial object.
200 * @param format The output format to set.
201 * @return Operation status.
202 */
203 GoFx(kStatus) GoSerial_SetSelcomFormat(GoSerial serial, GoSelcomFormat format);
204
205 /**
206 * Gets the current Selcom output format.
207 *
208 * @public @memberof GoSerial
209 * @version Introduced in firmware 4.0.10.27
210 * @param serial GoSerial object.
211 * @return The current Selcom output format.
212 */
213 GoFx(GoSelcomFormat) GoSerial_SelcomFormat(GoSerial serial);
214
215 /**
216 * Gets the list of Selcom format options.
217 *
218 * @public @memberof GoSerial
219 * @version Introduced in firmware 4.0.10.27
220 * @param serial GoSerial object.
221 * @return An array list of Selcom format options.
222 */
223 GoFx(kArrayList) GoSerial_SelcomFormatOptionList(GoSerial serial);
224
225 /**
226 * Returns the count of available Selcom protocol output format options.
227 *
228 * @public @memberof GoSerial
229 * @version Introduced in firmware 4.0.10.27
230 * @param serial GoSerial object.
231 * @return The count of available Selcom protocol output format options.
232 */
233 GoFx(kSize) GoSerial_SelcomFormatOptionCount(GoSerial serial);
234
235 /**
236 * Gets the Selcom format option at the specified index.
237 *
238 * @public @memberof GoSerial
239 * @version Introduced in firmware 4.0.10.27
240 * @param serial GoSerial object.
241 * @param index Selcom format option index.
242 * @return Selcom format option value.
243 */
244 GoFx(GoSelcomFormat) GoSerial_SelcomFormatOptionAt(GoSerial serial, kSize index);
245
246 /**
247 * Sets the Selcom protocol maximum data scale value.
248 *
249 * @public @memberof GoSerial
250 * @version Introduced in firmware 4.0.10.27
251 * @param serial GoSerial object.
252 * @param value Maximum data scale value to set.
253 * @return Operation status.
254 */
255 GoFx(kStatus) GoSerial_SetSelcomDataScaleMax(GoSerial serial, k64f value);
256
257 /**
258 * Gets the Selcom protocol data scale maximum value.
259 *
260 * @public @memberof GoSerial
261 * @version Introduced in firmware 4.0.10.27
262 * @param serial GoSerial object.
263 * @return Maximum data scale value.
264 */
265 GoFx(k64f) GoSerial_SelcomDataScaleMax(GoSerial serial);
266
267 /**
268 * Sets the Selcom protocol minimum data scale value.
269 *
270 * @public @memberof GoSerial
271 * @version Introduced in firmware 4.0.10.27
272 * @param serial GoSerial object.
273 * @param value Minimum data scale value to set.
274 * @return Operation status.
275 */
276 GoFx(kStatus) GoSerial_SetSelcomDataScaleMin(GoSerial serial, k64f value);
277
278 /**
279 * Gets the Selcom protocol data scale minimum value.
280 *
281 * @public @memberof GoSerial
282 * @version Introduced in firmware 4.0.10.27
283 * @param serial GoSerial object.
284 * @return Minimum data scale value.
285 */
286 GoFx(k64f) GoSerial_SelcomDataScaleMin(GoSerial serial);
287
288 /**
289 * Sets the delay from exposure until output is triggered, in units based on GoDomain.
290 * mm units when GoDomain is distance, uS units when GoDomain is time.
291 *
292 * @public @memberof GoSerial
293 * @version Introduced in firmware 4.4.4.14
294 * @param serial GoSerial object.
295 * @param delay k64s object.
296 * @return Operation status.
297 */
298 GoFx(kStatus) GoSerial_SetSelcomDelay(GoSerial serial, k64u delay);
299
300 /**
301 * Gets the output delay.
302 *
303 * @public @memberof GoSerial
304 * @version Introduced in firmware 4.4.4.14
305 * @param serial GoSerial object.
306 * @return The output delay (us or mm).
307 */
308 GoFx(k64u) GoSerial_SelcomDelay(GoSerial serial);
309
310 /**
311 * Gets the ASCII protocol output delimiter string.
312 *
313 * @public @memberof GoSerial
314 * @version Introduced in firmware 4.0.10.27
315 * @param serial GoSerial object.
316 * @return A pointer to the string representing the ASCII protocol output delimiter.
317 */
318 GoFx(kChar*) GoSerial_AsciiDelimiter(GoSerial serial);
319
320 /**
321 * Sets the ASCII protocol output delimiter string.
322 *
323 * @public @memberof GoSerial
324 * @version Introduced in firmware 4.0.10.27
325 * @param serial GoSerial object.
326 * @param string A pointer to the string representing the ASCII protocol output delimiter.
327 * @return Operation status.
328 */
329 GoFx(kStatus) GoSerial_SetAsciiDelimiter(GoSerial serial, const kChar* string);
330
331 /**
332 * Gets the ASCII protocol output terminator string.
333 *
334 * @public @memberof GoSerial
335 * @version Introduced in firmware 4.0.10.27
336 * @param serial GoSerial object.
337 * @return A pointer to the terminator representing the ASCII protocol output delimiter.
338 */
339 GoFx(kChar*) GoSerial_AsciiTerminator(GoSerial serial);
340
341 /**
342 * Sets the ASCII protocol output terminator string.
343 *
344 * @public @memberof GoSerial
345 * @version Introduced in firmware 4.0.10.27
346 * @param serial GoSerial object.
347 * @param string A pointer to the string representing the ASCII protocol output terminator.
348 * @return Operation status.
349 */
350 GoFx(kStatus) GoSerial_SetAsciiTerminator(GoSerial serial, const kChar* string);
351
352 /**
353 * Gets the ASCII protocol output invalid value string.
354 *
355 * @public @memberof GoSerial
356 * @version Introduced in firmware 4.0.10.27
357 * @param serial GoSerial object.
358 * @return A pointer to the string representing the ASCII protocol output invalid value.
359 */
360 GoFx(kChar*) GoSerial_AsciiInvalidValue(GoSerial serial);
361
362 /**
363 * Sets the ASCII protocol output invalid value string.
364 *
365 * @public @memberof GoSerial
366 * @version Introduced in firmware 4.0.10.27
367 * @param serial GoSerial object.
368 * @param string A pointer to the string representing the ASCII protocol output invalid value.
369 * @return Operation status.
370 */
371 GoFx(kStatus) GoSerial_SetAsciiInvalidValue(GoSerial serial, const kChar* string);
372
373 /**
374 * Gets the ASCII protocol output custom data format string.
375 *
376 * @public @memberof GoSerial
377 * @version Introduced in firmware 4.0.10.27
378 * @param serial GoSerial object.
379 * @return A pointer to the string representing the ASCII protocol output invalid value.
380 */
381 GoFx(kChar*) GoSerial_AsciiCustomDataFormat(GoSerial serial);
382
383 /**
384 * Sets the ASCII protocol output custom data format.
385 *
386 * @public @memberof GoSerial
387 * @version Introduced in firmware 4.0.10.27
388 * @param serial GoSerial object.
389 * @param string A pointer to the string representing the ASCII protocol output custom data format.
390 * @return Operation status.
391 */
392 GoFx(kStatus) GoSerial_SetAsciiCustomDataFormat(GoSerial serial, const kChar* string);
393
394 /**
395 * Sets the enabled state of the ASCII protocol custom data format.
396 *
397 * @public @memberof GoSerial
398 * @version Introduced in firmware 4.0.10.27
399 * @param serial GoSerial object.
400 * @param enabled kTRUE to enable and kFALSE to disable.
401 * @return Operation status.
402 */
403 GoFx(kStatus) GoSerial_EnableAsciiCustomFormat(GoSerial serial, kBool enabled);
404
405 /**
406 * Gets the enabled state of the ASCII protocol custom data format.
407 *
408 * @public @memberof GoSerial
409 * @version Introduced in firmware 4.0.10.27
410 * @param serial GoSerial object.
411 * @return kTRUE if enabled and kFALSE otherwise.
412 */
413 GoFx(kBool) GoSerial_AsciiCustomFormatEnabled(GoSerial serial);
414
415 /**
416 * Sets the current standard format mode.
417 *
418 * @public @memberof GoSerial
419 * @version Introduced in firmware 4.5.3.57
420 * @param serial GoSerial object.
421 * @param mode The new StandardFormatMode.
422 * @return Operation status.
423 */
424 GoFx(kStatus) GoSerial_SetAsciiStandardFormat(GoSerial serial, GoAsciiStandardFormatMode mode);
425
426 /**
427 * Gets the current standard format mode.
428 *
429 * @public @memberof GoSerial
430 * @version Introduced in firmware 4.5.3.57
431 * @param serial GoSerial object.
432 * @return The StandardFormatMode.
433 */
434 GoFx(GoAsciiStandardFormatMode) GoSerial_AsciiStandardFormat(GoSerial serial);
435
436 kEndHeader()
437 #include <GoSdk/Outputs/GoSerial.x.h>
438
439 #endif
GoSerial::GoSerial_SelcomFormatOptionAt
GoSelcomFormat GoSerial_SelcomFormatOptionAt(GoSerial serial, kSize index)
Gets the Selcom format option at the specified index.
GoSerial::GoSerial_AsciiCustomFormatEnabled
kBool GoSerial_AsciiCustomFormatEnabled(GoSerial serial)
Gets the enabled state of the ASCII protocol custom data format.
k32u
GoSerial::GoSerial_AsciiCustomDataFormat
kChar * GoSerial_AsciiCustomDataFormat(GoSerial serial)
Gets the ASCII protocol output custom data format string.
GoSerial::GoSerial_SetAsciiCustomDataFormat
kStatus GoSerial_SetAsciiCustomDataFormat(GoSerial serial, const kChar *string)
Sets the ASCII protocol output custom data format.
GoSerial::GoSerial_SourceCount
kSize GoSerial_SourceCount(GoSerial serial)
Gets the number of sources of the specified output type that are currently selected for transmission...
k64u
GoSerial::GoSerial_SelcomDelay
k64u GoSerial_SelcomDelay(GoSerial serial)
Gets the output delay.
GoSerial::GoSerial_AsciiDelimiter
kChar * GoSerial_AsciiDelimiter(GoSerial serial)
Gets the ASCII protocol output delimiter string.
kSize
GoSerial::GoSerial_SelcomDataScaleMin
k64f GoSerial_SelcomDataScaleMin(GoSerial serial)
Gets the Selcom protocol data scale minimum value.
GoSerial::GoSerial_RemoveSource
kStatus GoSerial_RemoveSource(GoSerial serial, kSize index)
Removes (de-selects) the source at the specified index.
GoSerial::GoSerial_EnableAsciiCustomFormat
kStatus GoSerial_EnableAsciiCustomFormat(GoSerial serial, kBool enabled)
Sets the enabled state of the ASCII protocol custom data format.
kChar
GoSerial::GoSerial_Protocol
k32u GoSerial_Protocol(GoSerial serial)
Returns the current Serial output protocol value.
GoSerial::GoSerial_SetProtocol
kStatus GoSerial_SetProtocol(GoSerial serial, k32u protocol)
Sets the Serial output protocol.
GoSerial::GoSerial_ProtocolOptionCount
kSize GoSerial_ProtocolOptionCount(GoSerial serial)
Gets the count of serial protocol options.
GoSerial::GoSerial_SetSelcomDataScaleMax
kStatus GoSerial_SetSelcomDataScaleMax(GoSerial serial, k64f value)
Sets the Selcom protocol maximum data scale value.
GoSerial::GoSerial_OptionAt
k32u GoSerial_OptionAt(GoSerial serial, kSize index)
Gets the source option at the specified index.
GoSerial::GoSerial_ProtocolOptionAt
k32u GoSerial_ProtocolOptionAt(GoSerial serial, kSize index)
Gets the serial protocol option at the specified index.
GoSerial::GoSerial_SelcomRateOptionList
kArrayList GoSerial_SelcomRateOptionList(GoSerial serial)
Gets the list of Selcom rate options.
GoSerial::GoSerial_SetSelcomDataScaleMin
kStatus GoSerial_SetSelcomDataScaleMin(GoSerial serial, k64f value)
Sets the Selcom protocol minimum data scale value.
GoSerial::GoSerial_SelcomFormatOptionList
kArrayList GoSerial_SelcomFormatOptionList(GoSerial serial)
Gets the list of Selcom format options.
GoSerial::GoSerial_AddSource
kStatus GoSerial_AddSource(GoSerial serial, k32u sourceId)
Selects the specified source for transmission.
GoSerial::GoSerial_OptionCount
kSize GoSerial_OptionCount(GoSerial serial)
Gets the number of source options.
GoSdkDef.h
Essential SDK declarations.
GoSerial::GoSerial_SetAsciiStandardFormat
kStatus GoSerial_SetAsciiStandardFormat(GoSerial serial, GoAsciiStandardFormatMode mode)
Sets the current standard format mode.
GoSerial::GoSerial_SelcomRateOptionCount
kSize GoSerial_SelcomRateOptionCount(GoSerial serial)
Returns the count of available Selcom protocol output rate options.
GoSerial::GoSerial_SelcomRate
k32u GoSerial_SelcomRate(GoSerial serial)
Gets the index of the currently selected Selcom output rate.
GoSerial::GoSerial_AsciiTerminator
kChar * GoSerial_AsciiTerminator(GoSerial serial)
Gets the ASCII protocol output terminator string.
GoSerial
Represents Serial output settings.
GoSerial::GoSerial_SelcomFormat
GoSelcomFormat GoSerial_SelcomFormat(GoSerial serial)
Gets the current Selcom output format.
GoSerial::GoSerial_AsciiInvalidValue
kChar * GoSerial_AsciiInvalidValue(GoSerial serial)
Gets the ASCII protocol output invalid value string.
GoAsciiStandardFormatMode
Represents an ASCII standard format type.
GoSerial::GoSerial_SelcomRateOptionAt
k32u GoSerial_SelcomRateOptionAt(GoSerial serial, kSize index)
Gets the Selcom rate option at the specified index.
GoSerial::GoSerial_SourceAt
k32u GoSerial_SourceAt(GoSerial serial, kSize index)
Gets the identifier of the selected output source at the specified index.
GoSerial::GoSerial_SetSelcomFormat
kStatus GoSerial_SetSelcomFormat(GoSerial serial, GoSelcomFormat format)
Sets the Selcom protocol output format.
GoSerial::GoSerial_SetSelcomRate
kStatus GoSerial_SetSelcomRate(GoSerial serial, k32u rate)
Sets the Selcom protocol output rate.
GoSerial::GoSerial_SetAsciiTerminator
kStatus GoSerial_SetAsciiTerminator(GoSerial serial, const kChar *string)
Sets the ASCII protocol output terminator string.
GoSerial::GoSerial_SetAsciiDelimiter
kStatus GoSerial_SetAsciiDelimiter(GoSerial serial, const kChar *string)
Sets the ASCII protocol output delimiter string.
GoSerial::GoSerial_SelcomFormatOptionCount
kSize GoSerial_SelcomFormatOptionCount(GoSerial serial)
Returns the count of available Selcom protocol output format options.
kArrayList
kObject
kStatus
GoSerial::GoSerial_ClearSources
kStatus GoSerial_ClearSources(GoSerial serial)
Removes all selected sources for the specified output type.
k64f
GoSerial::GoSerial_SetSelcomDelay
kStatus GoSerial_SetSelcomDelay(GoSerial serial, k64u delay)
Sets the delay from exposure until output is triggered, in units based on GoDomain.
GoSelcomFormat
Represents the selcom format followed on the serial output.
kBool
GoSerial::GoSerial_AsciiStandardFormat
GoAsciiStandardFormatMode GoSerial_AsciiStandardFormat(GoSerial serial)
Gets the current standard format mode.
GoSerial::GoSerial_SelcomDataScaleMax
k64f GoSerial_SelcomDataScaleMax(GoSerial serial)
Gets the Selcom protocol data scale maximum value.
GoSerial::GoSerial_SetAsciiInvalidValue
kStatus GoSerial_SetAsciiInvalidValue(GoSerial serial, const kChar *string)
Sets the ASCII protocol output invalid value string.