Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kArray1 GoGeoCal_YCenterFit | ( | GoGeoCal | cal,
|  | kSize | cameraIndex
| ) |  |

Gets Y center to Z fit.

The world Y center (mm) of an imager varies with the range if any pitch is present. It also represents the distance from the sensor reference 0 plane (usually mid-sensor). The fit is stored as polynomial coefficients. The Y center at a given Z range (mm) can be determined by:

      Y center = coefficients[0] + coefficients[1]*Z + ... + coefficients[N]*Z^N

Version
  Introduced in firmware 4.7.0.130

Parameters

  cal | GoGeoCal object.
  cameraIndex | Camera index. kERROR_PARAMETER if invalid.

Returns
  Array of Y center to Z fit coefficients. Type: k64f.