Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoPartDetection_SetThreshold | ( | GoPartDetection | detection,
|  | k64f | height
| ) |  |

Sets the part detection height threshold.

Note
  Supported with G2, G3

Version
  Introduced in firmware 4.0.10.27

Parameters

  detection | GoPartDetection object.
  height | The part detection height threshold value to set.(mm)

Returns
  Operation status.