Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetIntensityStepIndex | ( | GoSetup | setup,
|  | GoRole | role,
|  | kSize | index
| ) |  |

Sets the intensity step index.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which device to apply changes to. Use GO_ROLE_MAIN or GOROLE_BUDDYIDX(buddyidx). See GoRole for more details.
  index | The exposure step index to use for intensity acquisition.

Returns
  Operation status.

See also
  GoSetup_SetExposureMode, GoSetup_ExposureStepCount