Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSetup_SetActiveAreaZ | ( | GoSetup | setup,
|  | GoRole | role,
|  | k64f | value
| ) |  |

Sets the active area z origin.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which device to apply changes to. Use GO_ROLE_MAIN or GOROLE_BUDDYIDX(buddyidx). See GoRole for more details.
  value | Active area z origin (mm).

Returns
  Operation status.