Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k32u GoSetup_PatternSequenceIndexMax | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the current phase pattern index maximum value (inclusive).

Version
  Introduced in firmware 5.3.19.50

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from. Use GO_ROLE_MAIN or GOROLE_BUDDYIDX(buddyidx). See GoRole for more details.

Returns
  The current phase pattern index maximum value (inclusive).