Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensorInfo_ModelDisplayName | ( | GoSensorInfo | info,
|  | kChar * | modelDisplayName,
|  | kSize | capacity
| ) |  |

Gets the model display name of the sensor which provided the sensor information.

Version
  Introduced in firmware 5.3.17.23

Parameters

  info | GoSensorInfo object.
  modelDisplayName | A character array pointer.
  capacity | The character array capacity.

Returns
  Operation status.