Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_Cancel | ( | GoSensor | sensor | ) |

Aborts ongoing sensor communication.

This method asynchronously aborts ongoing communication; the next time that any I/O operation blocks for an extended period of time, it will be terminated. This method is thread-safe.

In order to resume communication, call GoSensor_Refresh or GoSensor_Connect.

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.

Returns
  Operation status.