Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

GoIntensityMode GoSetup_IntensityMode | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the intensity data generation mode.

Version
  Introduced in firmware 4.7.10.10

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from. Use GO_ROLE_MAIN or GOROLE_BUDDYIDX(buddyidx). See GoRole for more details.

Returns
  Intensity generation mode.