Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSurfaceGenerationFixedLength_SetStartTrigger | ( | GoSurfaceGeneration | surface,
|  | GoSurfaceGenerationStartTrigger | trigger
| ) |  |

Sets the fixed length surface generation start trigger.

Note
  Supported with G2, G3

Version
  Introduced in firmware 4.0.10.27

Parameters

  surface | GoSurfaceGeneration object.
  trigger | The surface generation start trigger value to set.

Returns
  Operation status.