Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoControl_GetVoltage | ( | GoControl | control,
|  | GoVoltageSetting * | voltage,
|  | k32u * | cableLength
| ) |  |

Get the sensor voltage settings (only on G3210)

Version
  Introduced in firmware 4.7.5.25

Parameters

  control | GoControl object.
  voltage | Destination to store voltage (can be kNULL)
  cableLength | Destination to store cable length (millimeters) (can be kNULL)

Returns
  Operation status.