Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_ResetEncoder | ( | GoSensor | sensor | ) |

Resets the encoder value.

NOTE: This is only possible with a direct encoder connection to a sensor. Resetting the encoder value when connected to a Master device will not work.

Version
  Introduced in firmware 4.5.3.57

Parameters

  sensor | GoSensor object.

Returns
  Operation status.