Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

k32u GoSetup_LayoutMultiplexingBank | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets Multiplex bank value being configured (may not be applicable or used) on device in n-buddy system.

Version
  Introduced in firmware 5.3.22.15

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from. Use GO_ROLE_MAIN or GOROLE_BUDDYIDX(buddyidx). See GoRole for more details.

Returns
  Multiplexing bank value.