Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoCylinderRegion_SetY | ( | GoCylinderRegion | region,
|  | k64f | value
| ) |  |

Sets the Y position.

Note
  Supported with G2, G3

Version
  Introduced in firmware 4.0.10.27

Parameters

  region | GoCylinderRegion object.
  value | The Y position to set.(mm)

Returns
  Operation status.