Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages

kStatus GoSensor_AlignmentReference | ( | GoSensor | sensor,
|  | GoAlignmentRef * | reference
| ) |  |

Gets the alignment reference of the sensor.

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.
  reference | A pointer that will hold the current alignment reference value.

Returns
  Operation status.