GoPxL SDK

- Home
- Files
- Namespace

GoSystem | ( | const kIpAddress & | address,
|  | k32u | port = `GO_PXL_SDK_DEFAULT_CONTROL_PORT`
| ) |  |
| explicit

Constructs a GoSystem object with the given IP address and control port number.

This constructor automatically creates a GoRestClient instance, and initialize the IP address and port the client should connect to when the Connect() API is called.

Version
  Introduced in 0.2.1.53.

Parameters

  address | The IPv4 address of the Gocator remote device.
  port | The IP control port number of the Gocator device. A port value of zero (0) is invalid.

Exceptions

  Go::Exception | If arguments are invalid.