Gocator API

- Home
- Topics
- Types
- Files

All Classes Files Functions Variables Typedefs Macros Modules Pages
Public Member Functions
GoRangeMsg Class Reference
GoSdk/Messages » Data Channel

## Description

Represents a data message containing a set of range data.

Note
  Supported with G1

Inheritance diagram for GoRangeMsg:

## Public Member Functions
kStatus | GoDataMsg_SetStreamStep (GoDataMsg message, GoDataStep streamStep)
| Sets the source of the data stream. More...
kStatus | GoDataMsg_SetStreamStepId (GoDataMsg message, k32s streamStepId)
| Sets the identifier of the data stream from the source. More...
GoDataStep | GoDataMsg_StreamStep (GoDataMsg message)
| Gets the source of the data stream. More...
k32s | GoDataMsg_StreamStepId (GoDataMsg message)
| Gets the identifier of the data stream from the source. More...
GoDataMessageType | GoDataMsg_Type (GoDataMsg message)
| Returns the message type for a data channel message given in a GoDataSet. More...
k16s * | GoRangeMsg_At (GoRangeMsg msg, kSize index)
| Gets a pointer to Range data. More...
kSize | GoRangeMsg_Count (GoRangeMsg msg)
| Gets the count of Range data in this message. More...
k32u | GoRangeMsg_Exposure (GoRangeMsg msg)
| Gets the exposure. More...
GoDataSource | GoRangeMsg_Source (GoRangeMsg msg)
| Gets the Range source. More...
k32s | GoRangeMsg_ZOffset (GoRangeMsg msg)
| Gets the Range z-offset, in micrometers. More...
k32u | GoRangeMsg_ZResolution (GoRangeMsg msg)
| Gets the Range z-resolution, in nanometers. More...

The documentation for this class was generated from the following file:

- Messages/GoDataTypes.h